Rename the unforce_h10.txt to force_h10.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will force to install the image openatv-6.3-zgemmah10combo-20210111_usb.zip in the linux1 selection
