Rename the unforce_hd60.txt to force_hd60.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will force to install the image openatv-7.6.0-ax60-20260801_multi.zip in the linux1 selection
