Rename the unforce_pulse4kmini.txt to force_pulse4kmini.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will then force the openatv-7.6.0-pulse4kmini-20260702_mmc.zip into the linux1 slot
